SECTION 105100
 (New SECTION 105113)

LOCKERS
(19000, 19100)

Display hidden notes to specifier. (Don't know how? Click Here) 
PART 1    GENERAL
1.1	SECTION INCLUDES

A.	Cell Phone Lockers. 

B.	Cell Phone Lockers with Front Access Panel. 

1.2	REFERENCES

A.	IBC - International Building Code.

1.3	RELATED SECTIONS

A.	Section 04800 - Masonry Assemblies.
B.	Section 05400 - Cold Formed Metal Framing: Framed wall openings to receive cell phone lockers.
C.	Section 06100 - Wood Framing: Framed wall openings to receive cell phone lockers.
D.	Section 09250 - Gypsum Board.

1.4	SUBMITTALS
A.	Submit under provisions of Section 013300.
B.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
D.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2008 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Cell phone locker components are shipped assembled. All finishes shall be protected from soiling and damage during handling.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of cell phone locker products that fail in materials or workmanship within 3 years from date of substantial completion.

PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Salsbury Industries, 1010 East 62nd Street; Los Angeles, CA 90001-1598; Toll Free Tel: 1-800-LOCKERS (1-800-562-5377); Fax: 1-800-562-5399; Email: salsbury@lockers.com; Website: www.lockers.com.
B.	Substitutions:  Not permitted.

2.2	CELL PHONE LOCKERS
Cell phone lockers and cell phone lockers with front access panel:  Constructed entirely of heavy duty aluminum; durable powder coated finish; both series are available with standard A doors or larger B doors and all doors include a clear plastic cardholder; can accommodate built-in combination locks, built-in key locks, combination padlocks, key padlocks or factory installed master keyed locks or resettable combination locks.

A.	Cell Phone Locker 19000 Series:
		1.	Surface Mounted.
			a.	7 door high units.
			b.	6 door high units.
			c.	5 door high units.
			e.	4 door high units.
			f.	3 door high units.
	2.	Recessed Mounted.
			a.	7 door high units.
			b.	6 door high units.
			c.	5 door high units.
			e.	4 door high units.
			f.	3 door high units.

B.	Cell Phone Locker with Front Access Panel 19100 Series:
1.	Surface Mounted.
		a.	7 door high units.
			b.	6 door high units.
			c.	5 door high units.
			e.	4 door high units.
			f.	3 door high units.
	2.	Recessed Mounted.
			a.	7 door high units.
			b.	6 door high units.
			c.	5 door high units.
			e.	4 door high units.
			f.	3 door high units.

C.	Unit Width:
1.	19000 Series – Surface Mounted.
a.	37 inches (940 mm).
b.	30-1/2 inches (775 mm).
c.	24 inches (610 mm).
d.	17-1/2 inches (445 mm).
2.	19000 Series – Recessed Mounted.
a.	35-3/4 inches (908 mm).
b.	29-1/4 inches (743 mm).
c.	22-3/4 inches (578 mm).
d.	16-1/4 inches (413 mm).
3.	19100 Series – Surface Mounted.
a.	37 inches (940 mm).
b.	30-1/2 inches (775 mm).
c.	24 inches (610 mm).
d.	17-1/2 inches (445 mm).
4.	19100 Series – Recessed Mounted.
a.	35-3/4 inches (908 mm).
b.	29-1/4 inches (743 mm).
c.	22-3/4 inches (578 mm).
d.	16-1/4 inches (413 mm).

D.	Unit Height:	
		1.	19000 Series – Surface Mounted.
a.	42 inches (1,067 mm).
b.	36-1/2 inches (927 mm).
c.	31 inches (787 mm).
d.	25-1/2 inches (648 mm).
e.	20 inches (508 mm).
		2.	19000 Series – Recessed Mounted.
a.	40-3/4 inches (1,035 mm).
b.	35-1/4 inches (895 mm).
c.	29-3/4 inches (755 mm).
d.	24-1/4 inches (616 mm).
e.	18-3/4 inches (476 mm).
		3.	19100 Series – Surface Mounted.
a.	42 inches (1,067 mm).
b.	36-1/2 inches (927 mm).
c.	31 inches (787 mm).
d.	25-1/2 inches (648 mm).
e.	20 inches (508 mm).
		4.	19100 Series – Recessed Mounted.
a.	40-3/4 inches (1,035 mm).
b.	35-1/4 inches (895 mm).
c.	29-3/4 inches (755 mm).
d.	24-1/4 inches (616 mm).
e.	18-3/4 inches (476 mm).

	E.	Unit Depth:	
		1.	19000 Series – Surface Mounted.
a.	Overall Depth.
i.	9-1/4 inches (235 mm).
				ii.	6-1/4 inches (159 mm).
b.	Compartment Depth.
i.	8 inches (203 mm).
				ii.	5 inches (127 mm).
		2.	19000 Series – Recessed Mounted.
a.	Overall Depth.
i.	8-3/4 inches (222 mm).
				ii.	5-3/4 inches (146 mm).
b.	Compartment Depth.
i.	8 inches (203 mm).
				ii.	5 inches (127 mm).
		3.	19100 Series – Surface Mounted.
a.	Overall Depth.
i.	9-1/4 inches (235 mm).
				ii.	6-1/4 inches (159 mm).
b.	Compartment Depth.
i.	8 inches (203 mm).
				ii.	5 inches (127 mm).
		4.	19100 Series – Recessed Mounted.
a.	Overall Depth.
i.	8-3/4 inches (222 mm).
				ii.	5-3/4 inches (146 mm).
b.	Compartment Depth.
i.	8 inches (203 mm).
				ii.	5 inches (127 mm).

	F.	Lock Type:
	1.	Master keyed locks.
	2.	Resettable combination locks.

G.	Unit Color:
	1.	Color: Aluminum - standard.
	2.	Color: Bronze - standard.
	3.	Color: Gold - standard.
	4.	Color: Sandstone – standard.

2.3	INTERIOR EQUIPMENT

A.	Standard Hardware Features: 
1.	2 inch (51 mm) wide x 5/8 inch (16 mm) high clear plastic cardholder
(card included).
2.	Master keyed locks or resettable combination locks.
3.	Front access panel lock (available with 19100 series cell phone lockers only).

2.4	OPTIONAL EQUIPMENT

A.	Cell Phone Locker Enclosures:  For use with select recessed mounted units only.

	1.	7 door high units.	
2.	6 door high units.
	3.	5 door high units.

a.	Unit Width:
	i.	5 door wide units:  37 inches (940 mm).
	ii.	4 door wide units:  30-1/2 inches (775 mm).
	iii.	3 door wide units:  24 inches (610 mm).

b.	Unit Height:
	i.	7 door high units:  66-1/2 inches (1,689 mm).
	ii.	5 door and 6 door high units:  61 inches (1,549 mm).

c.	Unit Depth:  9-1/4 inches (235 mm).

B.	Cell Phone Locker Pedestals:  For use with select surface mounted units only.

	1.	7 door high units.	
2.	6 door high units.
	3.	5 door high units.

a.	Unit Width:  22 inches (559 mm).

b.	Unit Height:
	i.	5 door high units:  30 inches (762 mm).
	ii.	6 door and 7 door high units:  24-1/2 inches (622 mm).

c.	Unit Depth:  10 inches (254 mm).

C.	Doors:
	1.	Identification:
		a.	Custom engraved placards.
		b.	Custom door engraving-regular fill.
c.	Custom door engraving-black fill.
	2.	Plexiglass window:  1-1/8 inch (29 mm) wide x 7/8 inch (22 mm) high.
	3.	Door slot:
		a.	A size door:  5-1/2 inches (140 mm) wide x 3/4 inch (19 mm) high.
		b.	B size door:  12 inches (305 mm) wide x 3/4 inch (19 mm) high.

D.	Locks:  All optional locking systems are factory installed.
	1.	Built-in spring latch combination locks.
	2.	Built-in spring latch key locks.
	3.	Combination padlock with built-in hasp
	4.	Key padlock with built-in hasp.
	5.	Built-in hasp for user provided padlock.

E.	Master keys:
	1.	Master control key for factory installed resettable combination locks.
	2.	Master control key for factory installed keyed lock.
3.	Master control key for factory installed built-in combination locks.
	4.	Master control key for factory installed built-in keyed locks.
	5.	Master control key for combination padlocks.

F.	Locker key wristband.

G.	Flexible grommet:  1 inch (25 mm) diameter.

H.	Custom unit finish:  Minimum order of ten (10) units.

I.	Custom door configuration:  Minimum order of ten (10) units.

J.	Custom unit depth:  Minimum order of ten (10) units.

K.	Custom rear access:  Minimum order of ten (10) units.
	1.	Removable rear cover panel.
	2.	Hinged rear cover panel.

2.5	CONSTRUCTION
A.	Locker Doors:  Fabricated from extruded heavy duty aluminum specially formed for added strength and rigidity.
1.	Doors:
a.	A Door – 11 gauge - .094 inch (2.38 mm) thick aluminum.
b.	B Door – 8 gauge - .125 inch (3.17 mm) thick aluminum.
2.	Single-Point Latch:  Made of stainless steel, securely fastened to door.
B.	Locker Body:  Heavy duty aluminum specially formed for added strength and rigidity and to ensure tight joints at fastening points.
C.	Hinges:
1.	A and B size standard doors:  Built-in continuous hinge.
2.	Front access panel (19100 series only):  Built-in continuous hinge.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding. 

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.  Clean surfaces with mild dish detergent.  Do not use harsh abrasive cleaners.  Lubricate locks with graphite type lubricants only.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industries’ installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before substantial completion.

END OF SECTION