SECTION 105100
 (New SECTION 105126)

LOCKERS
(92000, 93000, 94000, 95000, 98000, 90000)

Display hidden notes to specifier. (Don't know how? Click Here) 

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Plastic Lockers.

1.2	REFERENCES

A.	IBC - International Building Code.

1.3	RELATED SECTIONS
A.	Section 03300 (03 30 00) – Cast-in-Place Concrete:  Concrete bases.
B.	Section 06100 (06 10 00) – Rough Carpentry:  Wood ground and furring for anchoring lockers.
C.	Section 09650 (09 65 13.13) – Resilient Base.

1.4	SUBMITTALS
A.	Submit under provisions of Section 013300.
B.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
D.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2008 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.
D.	Do not deliver plastic lockers to the site until the building is enclosed and HVAC systems are in operation.  Deliver plastic lockers in manufacturer's original packaging.  Store in an upright condition. Protect plastic lockers from exposure to direct sunlight.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Salsbury Industries, 1010 East 62nd Street; Los Angeles, CA 90001-1598; Toll Free Tel: 1-800-LOCKERS (1-800-562-5377); Fax: 1-800-562-5399; Email: salsbury@lockers.com; Website: www.lockers.com.
B.	Substitutions:  Not permitted.

2.2	LOCKERS
Double-tier, triple-tier, four-tier, five-tier, eight-tier and ten-tier plastic lockers:  Constructed of water resistant high grade Acrylonitrile Butadiene Styrene (ABS) plastic that combines strength and durability; includes stainless steel hinges and a stainless steel hasp for locking; can accommodate combination padlocks or key padlocks.

A.	Plastic Locker Series:
1.	92000 series:  Double-tier.
2.	93000 series:  Triple-tier.
3.	94000 series:  Four-tier.
4.	95000 series:  Five-tier.
5.	98000 series:  Eight-tier.
6.	90000 series:  Ten-tier.

B.	Unit Width:  12-3/4 inches (324 mm).

C.	Unit Height:	
1.	73 inches (1,854 mm) with adjustable legs fully retracted.
2.	74 inches (1,880 mm) with adjustable legs fully extended.
	D.	Unit Depth:  18 inches (457 mm).

	E.	Unit Assembly:
		1.	Unassembled units (Knocked-down).
		2.	Assembled units.

F.	Color:
	1.	Door finish:
	a.	Color: Gray - standard.
		b.	Color: Tan - standard.
		c.	Color: Blue - standard.
2.	Body finish:  Dark gray.

2.3	INTERIOR EQUIPMENT

B.	Standard Hardware Features: 
	1.	Stainless steel padlock hasp.
		2.	Stainless steel door hinges.
3.	Coat rod (available with double-tier lockers only).

2.4	OPTIONAL EQUIPMENT

	A.	Sloping hoods.

B.	Compartment shelf (not available for 10-tier units only).

C.	Padlocks:
	1.	Combination padlocks.
	2.	Keyed padlocks.

D.	Master keys:  Master control key for combination padlocks.

E.	Engraved name/number plates.

2.5	CONSTRUCTION
A.	Locker Doors:  Constructed of water resistant high grade Acrylonitrile Butadiene Styrene (ABS) plastic.
	1.	Door:  1/4 inch (6.4 mm) thick ABS plastic.
	2.	Single-Point Latch:  Made of stainless steel, securely fastened to door.
B.	Locker Body:  Constructed of water resistant high grade Acrylonitrile Butadiene Styrene (ABS) plastic.  Frames assemble via an integral interlocking latching system.
C.	Hinges:  Self-closing hinge: 0.074 inch (1.88 mm) thick sheet steel, double spun, full loop, tight pin, securely fastened to the door and locker body.
1.	Double-tier lockers:  Four 2 inch (51 mm) high five-knuckle hinges.
2.	Triple-tier, four-tier & five-tier lockers:  Two 2 inch (51 mm) high five-knuckle hinges.
3.	Eight-tier & ten-tier lockers:  One 2 inch (51 mm) high five-knuckle hinge.
D.	Optional factory assembly of locker bodies.
2.6	MATERIALS
A.	High grade Acrylonitrile Butadiene Styrene (ABS) plastic formed under high pressure into solid plastic components.
B.	Stainless-Steel Sheet:  ASTM A 666, Type 304.
	C.	Fasteners: Tamper-Resistant Fasteners:  Stainless steel torx-head screws.
		1.	Locker Connectors:  No. 10-24 sex bolt.
2.	Anchors:  Type and size required for secure anchorage.
3.	Drilled-in-place Masonry Anchors: Minimum 1/4 by 1-3/4 inch (6 by 44 mm) screws.

2.7	LOCKER FABRICATION
A.	Locker box fabricated from interlocking injection moulded components made of Acrylonitrile Butadiene Styrene (ABS) plastic.
B.	Hardware Attachment:  All hinges, handles, hasps and ABS components attached with tamper-resistant screws.
C.	Provide ventilated panels where indicated.
D.	Adjustable Legs:  Set height from 73 inches (1,854 mm) to 74 inches (1,880 mm).
E.	Continuous Sloping Tops:  Fabricated in lengths indicated, without visible fasteners at splice locations; and finished to match lockers.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding. 

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industries’ installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION